EEE 183/262      	     WIRELESS COMMUNICATION SYSTEMS		   FALL  2026

Instructor	:  	Preetham B. Kumar
Website 	:	https://www.csus.edu/faculty/k/preetham.kumar/
Class schedule	:   	Tues: 3–4.15 pm, Riverside Hall 1002
				Thurs:3–4.15 pm, Zoom:    https://csus.zoom.us/j/83606628827
Office hours:   	Tues./Thurs.: 11 am – 12.30 pm or by appointment
https://csus.zoom.us/j/867091331
Office		:   	Riverside Hall 5006							
Telephone	:   	916-278-7949 
E-mail		:   	kumarp@ecs.csus.edu

Prescribed Text: 	‘Wireless Communications: Principles and Practice’ 
		by Theodore S. Rappaport, Cambridge University Press, Updated 2nd Edition, 2024. 
		ISBN: 9781009489843

References:		Student Edition of MATLAB/SIMULINK
		‘Modern Digital and Analog Communication Systems,’ by B.P. Lathi, 
		Z. Ding, Oxford University Press; 4th edition, 2009
Class format and grading

		Midterm I:	20%
			Midterm II:	20 %
	              	Finals:		30 % (comprehensive)
			Project:	20%
			Homework:	10% 
2 double-sided pages of notes are allowed for midterms 
4 double-sided pages of notes for final.
Top Hat
We will be using the Top Hat (www.tophat.com) classroom response system in class. You will be able to submit answers to in-class questions using Apple or Android smartphones and tablets, laptops, or through text message. 
You can visit the Top Hat Overview (https://success.tophat.com/s/article/Student-Top-Hat-Overview-and-Getting-Started-Guide) within the Top Hat Success Center which outlines how you will register for a Top Hat account, as well as providing a brief overview to get you up and running on the system.
An email invitation will be sent to you by email, but if you do not receive this email, you can register by simply visiting our course website: TBA
Note: our Course Join Code is TBA


Class Schedule for Fall 2026

	WEEK	        				       TOPICS			  CHAPTERS	_________________________________________________________________________
 		1		08/31/26		Introduction				1
		2		09/07/26		Cellular Concept-Fundamentals	3.1-3.7
		3,4		09/14/26		Mobile Radio Propagation		4.1-4.9
							Large Scale Path Loss
		5		09/28/26		Midterm I Review 
		6		10/05/26		Midterm I

		7		10/12/26		Mobile Radio Propagation		5.1-5.7
							Small Scale Fading			 
		8,9		10/19/26		Modulation Techniques for		6.1-6.10 (Review)
							Mobile Radio				6.11-6.12
		10	          	11/02/26		Equalization and Diversity 		7.1-7.5
												7.10-7.11
		11		11/09/26		Midterm II Review 
		12		11/16/26		Midterm II
		13		11/23/26		Multiple Access Techniques		9.1-9.4, 9.7 	
		14		11/30/26		Wireless Networking			10.1-10.10
		15		12/07/26		Review
				12/14/26		Finals week
				

MATLAB COMMANDS AND TOOLBOXES
		
System operating commands
PC based MATLAB can be opened by clicking on the MATLAB icon. The MATLAB prompt is >>, which indicates that commands can be started, either line by line, or by running a stored program. A complete program, consisting of a set of commands, can be stored in a MATLAB file for repeated use as follows:
(a)  Open a file in any text editor ( either in MATLAB or Word/Notepad/WordPad) and write the program.
(b)  After writing the program, save it  as a filename.m file. 
(c)  To run the program, click on the Run arrow, or type the filename after the prompt:
>> filename
The program will run, and the results/error messages, if any,  will be displayed on the screen. Plots will appear on a new screen.
I.  NUMBERS
  Generation of  numbers
  Example: Generate the real numbers z1 = 3, z2 = 4.
  >>  z1 = 3
  >>  z2 = 4
  Example: Generate the complex numbers z1 = 3+j4, z2 = 4+j 5
  >>  z1 = 3+4j
  >>  z2 = 4+5j
Note:  The symbol i can be used instead of j to represent  √-1.


Example:  Find the magnitude and phase of the complex number 3+j*4
>>  z = 3+j*4
>>  zm = abs(z)			; gives the magnitude of z
>>  zp = angle(z)			; gives the phase of z in radians
Addition or Subtraction of Numbers  (real or complex)
>>  z = z1 + z2			; addition
>>  z = z1 - z2				; subtraction
Multiplication or Division of Numbers (real or complex)
>>  z = z1*z2				; multiplication
>>  z = z1/z2				; division
II.  VECTORS
  Generation of  vectors
  Example: Generate the vectors x = [1 3 5] and y = [ 2 0 4 5 6]
  >>  x = [1 3 5]			 ; generates the vector of length 3
  >>  y = [2 0 4 5 6]			; generates the vector of length 5
Addition or Subtraction of Vectors x and y  of same length
>>  z = x+ y				; addition
>>  z = x - y				; subtraction
Multiplication or Division of Vectors x and y  of same length
>>  z = x. * y				; multiplication
>>  z = x. / y				; division
Note: The dot after x is necessary since x is a vector and not a number.



MATLAB TOOLBOXES

MATLAB commands are divided into different toolboxes depending on the applications. Various toolboxes developed by MATLAB include:
Communication Toolbox
Image Processing Toolbox
Signal Processing Toolbox 
Controls Toolbox
Spline Toolbox
Neural Network Toolbox 
Nonlinear Control Design Toolbox 
Statistics Toolbox 
Optimization Toolbox
Symbolic Math Toolbox 
Partial Differential Equation Toolbox 
PROGRAMMING WITH VECTORS
Programs involving vectors can be written using either FOR LOOPS or VECTOR commands. Since MATLAB is basically a vector-based program, it is often more efficient to write programs using VECTOR commands. However, FOR LOOPS give a clearer understanding of the program, especially for the beginner:
Example:  Sum the following series:
	S = 1 + 3 + 5  . . . . . . .99.
FOR LOOP approach
>>  S = 0.0;				; initializes the sum to zero
>>  for  i = 1 : 2 : 99;
	S = S + i;
      end;
>> S					; gives the value of the sum
VECTOR approach

>> i =1: 2 : 99;			; creates the vector i
>> S = sum ( i );			; obtains the sum S
Example:   Generate the discrete-time signal y(n) = n sin(n/2) in the interval 0  n  10.

FOR LOOP approach
>> for  n = 1:1: 11;
	n1 = n – 1;    		
	y(n) = n1 * sin(pi*n1/2);
     end;
>>  y					; gives the vector y
>> n = 0:1:10;				; generates the vector n
>> stem(n,y);				; plots the signal y vs. n with impulses

VECTOR approach
>> n = 0 : 10;				; creates the vector n
>> y = n.*sin(pi*n/2);			; obtains the vector y
>> stem(n,y)				; plots the signal y vs. n with impulses


SIMULINK COMMANDS AND EXAMPLES
After logging into MATLAB, you will receive the prompt  >>. In order to open up SIMULINK, either click on the SIMULINK icon or type in the following:
>> simulink
GENERAL SIMULINK OPERATIONS
Two windows will open up:  the model window and the library window. The model window is the space utilized for creating your simulation model. In order to create the model of the system, components will have to be taken from the library using the computer mouse and inserted into the model window. 
If you browse the library window, the following sections will be seen. Each section can be accessed by clicking on it.
· Sources - This section consists of different signal sources such as sinusoidal, triangular, pulse, random or files containing audio or video signals.
· Sinks  -  This section consists of measuring instruments such as scopes and displays
· Linear - This section consists of linear components performing operations like summing,    
      integration, product. 
· Nonlinear - Nonlinear operations
· Connections - Multiplexers, Demultiplexers
· Toolboxes - These specify different areas of SIMULINK
· Communications
· DSP
· Neural Nets
· Simulation Extras
EDITING, RUNNING AND SAVING SIMULINK FILES
The complete system is created in the model window by utilizing components from the various available libraries. Once a complete model is created, save the model  into a file. Click on Simulation and select Run. The simulation will run, and the output plots can be displayed by clicking on the appropriate sinks. Save the output plots also into files. The model and output files can be printed out from the files.
DEMO FILES
Try out the demo files, both in the main library window, and in the Toolboxes window. There are several illustrative demonstration files in the areas if signal processing, image processing and communications.
Simulation and graphical display of continuous-time signals and systems
Continuous-time system


 x(t) = A sin(t)

n(t)

Analog signal

Pseudo-random noise

Time scope
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Run the simulation for sinusoidal signal, x (t), amplitude of 5 Volts and frequency  = 10 rad./s. The signal n(t) is a pseudo-random noise with maximum amplitude of 0.5 volts. 
Observe the combined signal on the time scope and familiarize yourself with the settings. 
(b)  Try changing the sinusoidal signal amplitude (2V, 10V),  and frequency (20 rad./s, 50 rad./s), and observe the output on the time scope.
Discrete-time system

               +
    0.4
   z-1
   x(n)
   y(n)
  z/(z2+z-0.3)





(a) Observe the output signal on the time scope, for an input periodic pulse generator having the following parameters: Pulse amplitude 1 V, Pulse period 2 seconds and  pulse width of 1 second.
(b) Try changing the input signal amplitude (2 V, 3V) and  pulse width (0.5, 1.5 sec.) and observe on the time scope. 


